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· Question:
How to setup ​​AIW-343 under Ubuntu 18.04 on MIC-710AIX-00A1?

· Instructions :

In the beginning, we need to add runtime support for serial port manually using below commands.
# modprobe option
# echo 1bc7 1252 > /sys/bus/usb-serial/drivers/option1/new_id
*Please check module’s PID by command lsusb and replace it.
[image: ]
Remember to add a Mobile Broadband interface manually as following steps.
a. Go to Network Connection page and add a Mobile Broadband interface.
[image: ]
b. Click “Next”.
[image: ]

c. Select the correct country.
[image: ]
d. Select the correct provider.
`[image: ]
e. Select the plan which with correct APN.
[image: ]

f. Click “Apply”.
[image: ]
g. Click “Save”.
[image: ]
h. Finally, mobile broadband interface has been added.
[image: ]

Next, please follow below steps to make it execute automatically so that users don’t need to add runtime support for serial port manually each time after device reboot.

1. Create rc-local.service. 
# vi /etc/systemd/system/rc-local.service
Then add below contents.
[Unit]
Description=/etc/rc.local Compatibility
ConditionPathExists=/etc/rc.local
[Service]
Type=forking
ExecStart=/etc/rc.local start
TimeoutSec=0
StandardOutput=tty
RemainAfterExit=yes
SysVStartPriority=99
[Install]
WantedBy=multi-user.target

[image: ]
2. Create rc.local.
# vi /etc/rc.local
Then add below contents.
#!/bin/bash
modprobe option
[bookmark: _GoBack]echo 1bc7 <PID> > /sys/bus/usb-serial/drivers/option1/new_id
[image: ]
3. Modify permission of rc.local.
# chmod +x /etc/rc.local
4. Start the service.
# systemctl enable rc-local
# systemctl start rc-local

5. Check this item so that users don’t need to do anything then the cellular network will be established automatically after bootup.
[image: ]
6. Reboot and check whether cellular network established.
[image: ]

*Test environment:
[image: ]
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