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· Question:
[bookmark: OLE_LINK4][bookmark: OLE_LINK5]How to get binary code on u-center utility? 

· Instructions :

Step 1
Download u-center utility from u-blox’s website
	https://www.u-blox.com/en/product/u-center-windows

Step 2 
Install u-center utility at your desktop and connect GPS module to your host device

Step 3
	Select corresponding model on the section of receiver
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Step 4 
Check current GPS module version
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Step 5 
Assign specific Com port to connect GPS module on u-center utility
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Step 6
	Enable binary console to get binary code
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Step 7
	Enable “MON-HW” status message and check binary code
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Step 8
	Disable “MON-HW” status message and check binary code again
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Step 9
	Verify Binary code on linux platform and check the output message for sure
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T R R O e SGPTXT,01,01,01,NMEA unknown msg*58
,01,01,00, txbuf alloc*

SGPTXT,01,01,01,NMEA unknown msg*S8 $GPTXT,01,01,01,NMEA unknown msg*58
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P P AT (LD CETFes S$GPTXT,01,01,01,NMEA unknown msg*58
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*GPS_command_g108.txt (~/Desktop) - gedit

Open ~ save

\x00\X0A\x0B\x0C\x0D\XOE\X0F \x01\X00 az\ x03\XFF\X10\XFF\XFF\XFF\x36\x35\x05\x60\x4D\x00\x00\x00\x00\x80
\XF7\X00\x00\x00\x00\x00\X00\x76\x6B'> /dev/ttyACH®

cfg-ant
echo (39\x65\x62"> /dev/ttyACHO

AB'> /dev/

Status message

X06\x01\x03\ x00\ XBA\X09\XB1\X1E\X70'> /dev/ttyACH®
X05\x01\x02\x00\X06\x01\X0F\x38"> /dev/ttyACHD

01 03 00 0A 69 01 1E 70 enable message

01 02 00 06 01 OF 38

Disable HW Status message
[echo -ne '\xB5\x62\x66\x61\x03\x00\x0A\x09\x00\X1D\X6F ‘> /dev/ttyACHo
lecho -ne '\xB5\x62\x65\x01\x02\x00\x06\x01\x0F \x38'> /dev/tt

B5 62 06 01 03 00 OA 09 00 1D 6F
B5 62 05 01 02 00 06 01 OF 38
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