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· Question:
[bookmark: OLE_LINK4][bookmark: OLE_LINK5]How to verify EWM-G109H01E GPS Positioning on u-center utility?

· Instructions :

Step 1
Download “u-center utility”by following attached file and install both of module’s driver and utility before executing



Step 2
  Simply confirm following diagram on u-center to make sure if your GPS Positioning is done or not
[image: cid:image005.png@01D41E83.DD8D6FD0]
1. The field of fix mode is to check current module locates or not
Failure: “no fix” means
Success: the field will appear “2D”, “3D”wording in green color 
1. This icon is used to detect module relative position for current satellites which will mark in green color. 
1. This icon will display current signal quality of satellite (the value will be around 35~40 DB which may be easier to locate on your device) 

Step 3
For u-center utility, please reset the GPS module to factory default before verify GPS positioning feature 

(1)Connect to u-center utility by assigning COM port (pleas ensure the icon will change to green color for connecting successfully)
[image: cid:image008.jpg@01D41E8B.EF63CE90]
(2) Enter“F9”hotkey on keyboard and enable the message by clicking mouse right-clicking on 
following two options which mark in red arrow
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(3)Enter to the item of “UBX->CFG”,and select the option ”Revert to default configuration”,then click the “send” button in bottom left corner to activate it
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1. Erase previous GPS positioning by clicking this yellow icon
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(5)Switch back ”Save current configuration” option in item of “UBX->CFG” and click the “send” button in bottom left corner to activate it
[image: cid:image021.jpg@01D41E8B.EF63CE90]
1. Move your platform/device to open area which didn’t have shading object in the top of device
and the positioning action will be done after 1 minute later.
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Enabling an Intelligent Planet




